NOTES:
	8,15-		Cord clamp should be positioned so that 30mm of cord jacket extends above clamp.
9-	Seal to face commutator. Press to the tubing on armature shaft.
10-		To remove from shaft, place bearing in vise and crush outer race. Remove all internal bearing components so that
the inner race is all that is left. Use SRT320, Small Bearing Separator, to clamp the inner race and press off. 
Bearing presses to shoulder.
13-	Also order items 22 and 23.
	17,45-		Torque to 18-23 in-lbs.
	18-		Torque to 13 in./lbs.
	19-		Small diameter end to face commutator. Lightly lubricate before installing into field case.
	23-		Date Code located on nameplate or on underside of field case.
	26-		Press bearing until seated completely in pocket. Rubber seal to face spindle and gear assembly.
	29-		Press to bearing (item 10).
	40-		Torque to 20-25 in-lbs.
	50-		Press flush with surface facing spindle and gear assembly.

LUBRICATION:
Distribute 8 grams (.28 oz) of Polyrex grease in gear case. Coat clutch faces with approximately 3 grams (.17 oz) of clutch grease.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.